“Short” Product Specification

For

DSM Portable Gun Boxes

By Spacesaver

(Model#s EDPGB1594 AND EDPGB1596)

MANUFACTURERS

The products listed herein are based on a specific manufacturer to establish a standard of quality and minimum requirements. The drawings and specifications are based upon Portable Gun Box (EDPGB) as manufactured by Spacesaver. Products by any other manufacturers will be considered provided they comply with technical requirements and match the specified product in layout, configuration, construction appearance and finish, in accordance with the design concept and intent and must be approved by the department.

Manufacturer is subject to compliance with requirements for products provided by the following:

**Spacesaver Intermountain, 249 South 400 East, Salt Lake City, UT 84111. 801-363-5882**

# MATERIALS

18, 16 and 12 gauge cold rolled steel sheet: ASTM A1008, commercial quality, cold rolled carbon sheet steel, stretcher leveled, or roller leveled to stretcher leveled flatness, free of buckling, scale and surface imperfections.

Fasteners; zinc-plated or nickel plated steel; spotless-type exposed bolt heads; self locking nuts or lock washers for nuts on moving parts.

Hardware and equipment; Manufacturers standard product.

# PORTABLE GUN BOXES

General; body, door, internal body and lock parts to be made of cold rolled steel. All steel to be free from imperfections and capable of accepting a high-grade powder coat finish. The surfaces of the steel shall be cleaned thoroughly in a multi-stage process to inhibit corrosion and increase the durability of the applied finish. All un-plated parts shall then be finished with a minimum of 2 mil of powder coat paint.

# LOCKING DEVICES

Provide a DSM pad-lockable Slide Lock™ with at least 3 interlocking elements to resist forced attack. Locking device manufactured using a cold rolled steel billet, machined to a tight tolerance and zinc plated. Provide a hardened and zinc plated core that resists sawing attack.

# BODY AND LID

Welded modular construction; form each from a single piece, 18 gauge .048-inch cold rolled steel. Fabricated to form tight joints, with all joints and corners welded solid and ground smooth prior to painting.

# ACCESSORIES

Retractable handle; provide an ergonomically designed handle that retracts into the unit in such a way that does not increase the overall size of the unit when retracted. Provide a knurled aluminum handgrip.

Foam interior; provide a two-piece 6070 CH foam interior for cushioning of contents.

# WARRANTY

Provide the manufacturers 5 year limited parts and labour warranty.

# APPROVED MANUFATURER

**Spacesaver Intermountain, 249 South 400 East, Salt Lake City, UT 84111. 801-363-5882**