“Short” Product Specification

For

DSM Long Gun Cabinet and Accessory Boxes

By Spacesaver

(Model#s EDGC4, EDGC6, EDGC8, EDGC12, EDAB16 and EDAB20)

MANUFACTURERS

The products listed herein are based on a specific manufacturer to establish a standard of quality and minimum requirements. The drawings and specifications are based upon Upright Long Gun Cabinets and Accessory Cabinets (EDGC & EDAB series) as manufactured by Spacesaver Corporation (1-800-255-8170). Products by any other manufacturers will be considered provided they comply with technical requirements and match the specified product in layout, configuration, construction appearance and finish, in accordance with the design concept and intent and must be approved by the department.

Manufacturer is subject to compliance with requirements for products provided by the following:

**Spacesaver Intermountain, 249 South 400 East, Salt Lake City, UT 84111. 801-363-5882**

# MATERIALS

16 gauge cold rolled steel sheet: ASTM A1008, commercial quality, cold rolled carbon sheet steel, stretcher levelled, or roller levelled to stretcher levelled flatness, free of buckling, scale and surface imperfections.

Fasteners; zinc-plated or nickel plated steel; spotless-type exposed bolt heads; self locking nuts or lock washers for nuts on moving parts.

Hardware and equipment; Manufacturers standard plated product.

# UPRIGHT LONG GUN LOCKER

General; body, door, internal body and lock parts to be made of cold rolled steel. All steel to be free from imperfections and capable of accepting a high-grade powder coat finish. The surfaces of the steel shall be cleaned thoroughly in a multi-stage process to inhibit corrosion and increase the durability of the applied finish. All un-plated parts shall then be finished with a minimum of 2 mil of powder coat paint.

# LOCKING DEVICES

Provide a key locking, chromium plated “Tee” handle and three-point latch. Provide a pad lockable hasp that will accept a customer-supplied padlock.

# ACCESSORY BOXES

General; body, door, internal body and lock parts to be made of cold rolled steel. All steel to be free from imperfections and capable of accepting a high-grade powder coat finish. The surfaces of the steel shall be cleaned thoroughly in a multi-stage process to inhibit corrosion and increase the durability of the applied finish. All un-plated parts shall then be finished with a minimum of 2 mil of powder coat paint.

# LOCKING DEVICES

Provide a key locking “Tee” handle. Provide a pad lockable hasp that will accept a customer-supplied padlock.

# BODY AND DOOR

Welded modular construction; 16 gauge .0598-inch cold rolled steel. fabricated to form tight joints, with all joints and corners welded solid and ground smooth prior to painting. Comply with the following:

1. Door hinge shall be of the integral type, formed into the body

and door, joined with a 1/8-inch pin. The hinge shall be the full length of the door.

1. Provide a 20 gauge .0359-inch door stiffener welded to the door using “resistance” welding.
2. Provide pre-drilled mounting holes in the bottom & back of all cabinets.

# ACCESSORIES

Provide a 16 gauge .0598-inch shelf on model No.’s EDGC8, EDGC12, EDAB16 and EDAB20.

Provide Foam barrel supports and butt cushions on all Long Gun Cabinets.

**WARRANTY**

Provide the manufacturers 5 year limited parts and labour warranty.

# APPROVED MANUFATURER

**Spacesaver Intermountain, 249 South 400 East, Salt Lake City UT 84111. 801-363-5882.**