**“Short” Product Specification**

**For**

**DSM Safety Boxes**

**By Spacesaver**

# (Model#s SB138300, SB 138301, SB 138500, SB 138501, SB 171760,

# SB 161280, SB 201480 and SB241812

**MANUFACTURERS**

The products listed herein are based on a specific manufacturer to establish a standard of quality and minimum requirements. The Drawings and Specifications are based upon metal Footlockers “Safety Box II”, as manufactured by Spacesaver Corporation. Products by any other manufacturers will be considered provided they comply with technical requirements and match the specified product in layout, configuration, construction, appearance and finish, in accordance with the design concept and intent and must be approved by the Department.

Manufacturer is subject to compliance with requirements, for products provided by the following:

## Spacesaver Intermountain, 249 South 400 East, Salt Lake City, UT 84111. 801-363-5882

### MATERIALS

12 and 14 gaugesheet steel: commercial quality, stretcher leveled, or roller leveled to stretcher-leveled flatness, free of buckling, scale and surface imperfections.

Hardware and Equipment; Manufacturer’s standard plated product.

**FOOTLOCKERS**

General; Footlockers shall be made of .1046-inch 12 gauge and .0747-inch 14 gauge steel. All steel to be free from imperfections and capable of taking a high-grade powder coat finish. The surfaces of the steel shall be cleaned thoroughly in a multi-stage process to inhibit corrosion and increase the durability of the applied finish. All parts shall then be finished with a powder coat finish. Finish shall be baked on. All component parts and accessories shall be the same finish.

**DOOR**

Formed and welded construction, ground & polished corners, .1046-inch

12 gauge steel. Comply with the following:

1. Provide formed hasp protectors, angled & welded in place.
2. Provide anti-pry lip on three sides.

**BODY**

Formed and welded modular construction, ground & polished corners, .0747-inch 14 gauge steel. Comply with the following:

1. Provide a hardened steel hasp by ABUS™ # 02055 to accept a

customer supplied pad lock.

1. Provide formed safety edging on four sides.
2. Provide a carrying handle.

**HINGES**

Steel, heavy duty, continuous, piano hinge 1.5-inch open, .062-inch thick, 1/8-inch pin, 1/2-inch knuckle: full height of door, assembled to prevent the removal of the pin. Weld to door and body using metal/inert gas welding and resistance welding.

**FOOTLOCKER OPTIONAL ACCESSORIES**

Optional foam interior, mounting plate and MEDECO™ padlock.

# WARRANTY

Provide the manufacturers 5 year limited parts and labour warranty.

**APPROVED MANUFACTURER**

**Spacesaver Intermountain, 249 South 400 East, Salt Lake City, UT 84111. 801.363.5882**